Name:         2/3/4/6 GB Firmware Utility
Version:      1.0
Released:     November 20, 1997
Requires:
This utility is used to update the firmware on 2, 3, 4, and
6 GB SCSI hard drives in some Power Macintosh configurations
with firmware versions other than 0F0J. This utility can be
used on international versions of Mac OS as well as U.S. Mac
OS versions.
Description:
This bootable disk image contains a utility to fix a problem
with a limited number of 2, 3, 4, and 6 GB SCSI hard drives
in some Power Macintosh and Performa configurations that may
experience a problem waking after the machines has been set
to the Sleep mode.

This software consists of a Disk Copy NDIF (New Disk Image
Format) compressed image, which requires Disk Copy 6.1 or
later to use. Download this software to your hard drive and
then double-click it to use it. Disk Copy is available in
the Utilities folder.

Disk Copy 6.1 (or later) or Disk Image Mounter 2.1 (or
later) from Apple are the recommended applications to access
all disk images released by Apple and are the only supported
applications to access NDIF disk images.

Note: This utility supercedes the 2 GB/4 GB Download Utility
Version 1.0.


