Determines how many ticks must pass between contrail emissions. Contrails generally take the form of puffs of smoke emitted as exhaust at periodic intervals. This property does not apply to laser projectiles.
